**Common Logger32 soundcard macros**

|  |  |
| --- | --- |
| Macro | Action |
| $transmit$ | Start transmitting the TX buffer |
| $receive$ | End transmission, go to receive |
|  |  |
| $call$ | Callsign of the guy I am working from the log entry window |
| $myCall$ | My callsign (reset by right click in entry field 🡪 Change operator) |
| $name$ | Name of the guy I am working from the log entry window |
| $sentRST$ | RST of the guy I am working from the log entry window |
|  |  |
| $receivedRST$ | RST he sent me, from the log entry window |
| $receivedGrid$ | Locator he sent me, from the log entry window |
|  |  |
| $longDate$ | UTC date as dd-mm-yyyy *e.g*. 31-12-2012 |
| $longTime$ | UTC time as hh:mm:ss *e.g*. 02:33:54 |
| $longDateAndTime$ | UTC date & time as dd-mm-yyyy hh:mm:ss |
|  |  |
| $mode$ | Current mode from log entry window |
| $band$ | Current band, taken from the log entry window |
| $loop$ | Wait a few seconds then repeat this memory (escape or start entering call info to stop it repeating; use another $loop$ for longer delay between repeats) |
|  |  |
| $serialNumber$ | Serial number from # field in lower status bar (reset using # button) |
|  |  |
| $log$ | Complete a QSO, writing the QSO info to the log and clearing the log entry form ready for the next |
|  |  |
| $MMVARImode06$ | Change to PSK31 mode |
| $MMVARImode09$ | Change to RTTY mode |

*v1.0 June 2012 ZL2iFB* *Gary@G4iFB.com* *Many more commands & info in L32 help!*